AcousticQuantilePlot    Plot acoustic quantile
AcousticWeightingTable
                        Weighting acoustic table
AcuDNPercentile         Calculate reverse Percentile for period
AcuPercentile           Calculate reverse Percentile
ExtractIndexMark        Extract index and name of markers
HolidaysDate            Calculate Holidays date (Gregorian calendar)
HourlyEmean             Calculate hourly energetic mean
IntrusiveIndex          Calculate Intrusive Index (UNI/TS 11844 march
                        2022)
LdenCalculator          Calculate daily or total Lden
                        (Day-evening-night level)
Maskapply               Add index and name of markers in misure
                        dataframe
P1FA                    Noise data of misure in house open window
                        condition
P1FC                    Noise data of misure in house close window
                        condition
PTFA                    Noise data of misure in house open window
                        condition
PTFC                    Noise data of misure in house close window
                        condition
PlotNoiseTHcompare      Plot time history and compare frequency
                        components
PlotNoiseTimeHistory    Plot time history of noise misure with marker
                        and running Leq
PlotSpectrogram         Plot spectrogram
RoundTo                 Round to Multiple
SELcalc                 Calculate SEL (Single Event Level)
avr.day.night           Calculate daily and nightly energetic mean
                        period
dataset_impulsive1      Noise dataset of impulsive event (100 ms
                        acquisition time)
dataset_impulsive2      Noise dataset of impulsive event (100 ms
                        acquisition time)
dbsum                   Calculate energetic sum or difference of values
deco.time               Time decomposition
dfBW                    Table's 1/3 octave bandwidth
dfImpulsiveTrasform     Trasform impulsive dataframe (100 ms samples)
                        in dataframe (1s samples)
energetic.mean          Logarithmic mean
energetic.min           Function that calculate min value
energetic_w.mean        Weigth logaritmic mean
exampleHourlyData       Noise hourly data of misure in environmental
                        open space
iso                     Parameters table of equal loudness curve A (ISO
                        226:1987 “Acoustics - Normal
                        equal-loudness-level contours”)
markers                 Dataset with markers
runningLeq              Calculate running Leq
search.tone             Function research pure tone
searchImpulse           Search impulsive event
